Class 117 (75h) TBEN-LG-8DIP-8DOP
Attribute | Description | Access Type | Data Type | Values
113 (71h) | Digital In - Input value | Get | DWORD | 0 - "Channel 0", 1 - "Channel 1", 2 - "Channel 2", 3 - "Channel 3", 4 - "Channel 4", 5 - "Channel 5", 6 - "Channel 6", 7 - "Channel 7"
115 (73h) | Digital Out - Output value | Get | DWORD | 0 - "Channel 8", 1 - "Channel 9", 2 - "Channel 10", 3 - "Channel 11", 4 - "Channel 12", 5 - "Channel 13", 6 - "Channel 14", 7 - "Channel 15"
121 (79h) | Overcurrent VAUX | Get | DWORD | 0 - "Channel 0", 1 - "Channel 1", 2 - "Channel 2", 3 - "Channel 3", 4 - "Channel 4", 5 - "Channel 5", 6 - "Channel 6", 7 - "Channel 7"
119 (77h) | Digital Out - Overcurrent | Get | DWORD | 0 - "Channel 8", 1 - "Channel 9", 2 - "Channel 10", 3 - "Channel 11", 4 - "Channel 12", 5 - "Channel 13", 6 - "Channel 14", 7 - "Channel 15"
127 (7Fh) | Digital In - Invert digital input | Get/Set | DWORD | 0 - "Channel 0", 1 - "Channel 1", 2 - "Channel 2", 3 - "Channel 3", 4 - "Channel 4", 5 - "Channel 5", 6 - "Channel 6", 7 - "Channel 7"
137 (89h) | Digital Out - Manual reset after overcurr. | Get/Set | DWORD | 0 - "Channel 8", 1 - "Channel 9", 2 - "Channel 10", 3 - "Channel 11", 4 - "Channel 12", 5 - "Channel 13", 6 - "Channel 14", 7 - "Channel 15"
149 (95h) | Digital In 0 - Pulse stretching | Get/Set | USINT |
150 (96h) | Digital In 1 - Pulse stretching | Get/Set | USINT |
151 (97h) | Digital In 2 - Pulse stretching | Get/Set | USINT |
152 (98h) | Digital In 3 - Pulse stretching | Get/Set | USINT |
153 (99h) | Digital In 4 - Pulse stretching | Get/Set | USINT |
154 (9Ah) | Digital In 5 - Pulse stretching | Get/Set | USINT |
155 (9Bh) | Digital In 6 - Pulse stretching | Get/Set | USINT |
156 (9Ch) | Digital In 7 - Pulse stretching | Get/Set | USINT |