Class 117 (75h) TBEN-LG-16DIP
Attribute | Description | Access Type | Data Type | Values
113 (71h) | Digital In - Input value | Get | DWORD | 0 - "Channel 0", 1 - "Channel 1", 2 - "Channel 2", 3 - "Channel 3", 4 - "Channel 4", 5 - "Channel 5", 6 - "Channel 6", 7 - "Channel 7", 8 - "Channel 8", 9 - "Channel 9", 10 - "Channel 10", 11 - "Channel 11", 12 - "Channel 12", 13 - "Channel 13", 14 - "Channel 14", 15 - "Channel 15"
121 (79h) | Overcurrent VAUX | Get | DWORD | 0 - "Channel 0", 1 - "Channel 1", 2 - "Channel 2", 3 - "Channel 3", 4 - "Channel 4", 5 - "Channel 5", 6 - "Channel 6", 7 - "Channel 7"
127 (7Fh) | Digital In - Invert digital input | Get/Set | DWORD | 0 - "Channel 0", 1 - "Channel 1", 2 - "Channel 2", 3 - "Channel 3", 4 - "Channel 4", 5 - "Channel 5", 6 - "Channel 6", 7 - "Channel 7", 8 - "Channel 8", 9 - "Channel 9", 10 - "Channel 10", 11 - "Channel 11", 12 - "Channel 12", 13 - "Channel 13", 14 - "Channel 14", 15 - "Channel 15"
149 (95h) | Digital In 0 - Pulse stretching | Get/Set | USINT |
150 (96h) | Digital In 1 - Pulse stretching | Get/Set | USINT |
151 (97h) | Digital In 2 - Pulse stretching | Get/Set | USINT |
152 (98h) | Digital In 3 - Pulse stretching | Get/Set | USINT |
153 (99h) | Digital In 4 - Pulse stretching | Get/Set | USINT |
154 (9Ah) | Digital In 5 - Pulse stretching | Get/Set | USINT |
155 (9Bh) | Digital In 6 - Pulse stretching | Get/Set | USINT |
156 (9Ch) | Digital In 7 - Pulse stretching | Get/Set | USINT |
157 (9Dh) | Digital In 8 - Pulse stretching | Get/Set | USINT |
158 (9Eh) | Digital In 9 - Pulse stretching | Get/Set | USINT |
159 (9Fh) | Digital In 10 - Pulse stretching | Get/Set | USINT |
160 (A0h) | Digital In 11 - Pulse stretching | Get/Set | USINT |
161 (A1h) | Digital In 12 - Pulse stretching | Get/Set | USINT |
162 (A2h) | Digital In 13 - Pulse stretching | Get/Set | USINT |
163 (A3h) | Digital In 14 - Pulse stretching | Get/Set | USINT |
164 (A4h) | Digital In 15 - Pulse stretching | Get/Set | USINT |